**280W final checklist**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Model# | Lot# | Build # | Serial Number | Date of Mfg. | Shipped Firmware Rev |
| 280W |  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Action | Process | Mark | Notes |
|  | Basic mechanical check | All connectors, screws, screw caps, and bolts are installed and tight. |  |  |
|  | Verify | Be sure the Firmware is the latest, if not then upgrade to the current firmware revision. |  |  |
|  | Verify | Verify the single button functions through all menus. |  |  |
|  | Verify | Verify that the display screen functions normally. |  |  |
|  | Verify | Check for corrosion (especially the brass). |  |  |
|  | Verify | Verify all cables are correctly marked. |  |  |
|  | Verify | Check flow tube for debris (paint, excess Teflon tape, etc.). |  |  |

|  |  |  |
| --- | --- | --- |
| Name | Date | Initials |
|  |  |  |