**1XXEM meter final checklist**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Model# | Lot# | Build # | Serial Number | Date of Mfg. | Shipped Firmware Rev |
| 1XXEM |  |  |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Action | Process | Mark | Notes |
|  | Basic mechanical check | All connectors, screws, and bolts are installed and tight. |  |  |
|  | Verify | Verify all keyboard keys function. |  |  |
|  | Verify | Verify that the display screen functions normally, and that the backlight also functions. |  |  |
|  | Check Option | Verify 485 bus communications. |  |  |

|  |  |  |
| --- | --- | --- |
| Name | Date | Initials |
|  |  |  |